205

0

INTRODUCTION

Date: {{date}}

|  |
| --- |
| **{{client\_name}}** |
| **{{client\_address}}** |
| {{client\_city}} |

TO,

YES /{{m}} –{{y}}/{{id}}

KIND ATTN: - Sir,

**Sub:** Requirement of **Auto {{type}} Lift,** for your site **{{site\_name}} At {{client\_city}}.**

We are pleased to introduce ourselves as **An ISO 9001:2008 Certified Company &** one of the leading and dynamic manufacturer in the elevators industry. A Company who has maintenance experiences of all types and makes.

Hundreds of lifts are in operation all over Maharashtra, Karnataka, and Goa States. as well with capacity from 03 to 50 passengers. We have ultra-modern machines with testing equipment’s for manufacturing of vital components of lift. The direction switches used in our lifts are being manufactured by our CE certified venders to avoid mechanical wear and tear and reduces failure frequency of our lift. This increases the Mean Time between Failures of lift.

* Auto lift
* Variable speed, (V3F Drive)
* M.S. Collapsible, Wooden/MS Swing, Imperforated & Telescopic doors.
* Car with M.S. / S.S. / Wooden Laminated interior

Highlights of “Yes”Elevators

* Committed delivery performance.
* Customize Pricing.
* Round the clock after sales service made available.
* User-friendly Control Panel designed to sustain voltage fluctuations.
* Adequate, Skill & Qualified manpower as per P.W.D. norms
* Confirms to Indian standard and national building code.

For more information, please contact : 8055500071

**mail.id:-yeselevators@gmail.com**

**Thanking You.**

**For Yes elevators**

(Marketing Department)

**TECHNICALSPECIFICATION SHEET**

YES /{{m}} –{{y}}/{{id}}

|  |
| --- |
|  |

|  |  |  |
| --- | --- | --- |
| SR.NO | DISCRIPTION | SPECIFICATION |
| 1. | **TYPE** | **AUTO {{type}} LIFT** |
| 2. | **LOAD** | **{{capacity}} PASSENGER, {{weight}} KG.** |
| 3. | **SPEED** | **VARIABLE SPEED {{speed}} m/sec** |
| 4. | **CONTROLLER** | **INTEGRATED CONTROL PANEL** |
| 5. | **POWER SUPPLY** | **415 VOLT,03 PHASE,50 HZ AC** |

|  |  |  |
| --- | --- | --- |
| SHAFT DETAILS | | |
| 6. | **CAR TRAVEL** | **{{floors}}** |
| 7. | **HEIGHT** | **{{height}} METER (APPROX)** |
| 8. | **STOP / OPENING** | **{{stops}}/{{opening}}** |
| 9. | **SHAFT SIZE** | **WIDTH:-{{width}} X DEPTH:-{{depth}} MM** |
| 10. | **M/C ROOM** | **NA** |
| 11. | **PIT DEPTH** | **1500 MM** |
| 12. | **OVERHEAD** | **4600 MM** |

|  |  |  |
| --- | --- | --- |
| CAR DETAILS | | |
| 13. | **CAR SIZE INTERNAL** | **WIDTH :-{{car\_width}} MM / DEPT:-{{car\_depth}} MM** |
| 14. | **CAR OPENING** | **{{car\_opening}} MM X 2000 MM** |
| 15. | **CAR DOOR** | **{{door\_type}} OPENING AUTO DOOR** |
| 16. | **CAR PANEL** | **{{cabin\_type}} CABIN** |
| 17. | **CAR FLOORING** | **PVC FLOORING & FALL CEILING WITH BLOWER & LED LIGHT FITTING.** |

|  |  |  |
| --- | --- | --- |
| LIFT ENTRANCE | | |
| 18. | **LANDING DOOR** | **{{door\_type}} OPENING AUTO DOOR WITH DOOR FRAME** |
| 19. | **CLEAR OPENING** | **{{car\_opening}} MM X 2000 MM** |
| 20. | **ROPE** | **SELF LUBRICATED M.S ROPES** |

|  |  |  |
| --- | --- | --- |
| MACHINE DETAILS | | |
| 21. | **MACHINE TYPE** | **P.M.S.M (GEARLESS) MACHINE** |
| 22. | **POWER SUPPLY** | **415 VOLT,03 PHASE,50 HZ AC -** |

|  |  |
| --- | --- |
| ADDITIONAL FEATURES | |
| 1. | **UP / DOWN DIRECTION INDICATOR** |
| 2. | **FLOOR INDICATION** |
| 3. | **LIGHT & ALARM** |
| 4 | **ARD SYSTEM** |
| 5 | **INTERCOM SYSTEM** |
|  |  |

**Accepted byProposed by**

**OWNER OF LIFT For Yes elevators**

**(**Authorized Signatory) (Marketing Department)

YES /{{m}} –{{y}}/{{id}}

Date: {{date}}

**SUBJECT: QUOTATION** FOR **LIFT AT {{city}}.**

Dear Sir,

**QUOTATION** PRICE FOR SUPPLY & INSTALLATION OF ELEVATORS , AS GIVEN IN OUR ENCLOSED SPECIFICATION PAGE IS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| No | SPECIFICATION OF ELEVATORS | RATE/UNIT | QTY | AMOUNT |
| 1.  2.  3.  4.  5.  6. | AUTO {{type}} LIFT ({{floors}})  08 PASSENGERS, 544 KG.  {{cabin\_type}} CABIN  LANDING DOOR- {{door\_type}} OPENING AUTO DOOR  CAR ENTRANCE- {{door\_type}} OPENING AUTO DOOR  V. V. V. F. DRIVE  INTEGRATED CONTROL PANEL  **ARD** | **{{rate}}/-** | **{{qty}}** | **{{amt}}** |

RUPEES

{{amount\_in\_words}}

1. GST Extra.(18%)
2. **PWD permission, Inspection, license processing Fees Rs.28,000/- extra.**

PAYMENT TERMS:-

10% Advance against Order.

40% On intimation for material manufacturing.

40% Before dispatch of all material.

10% On testing of the lift

**Accepted by Proposed by**

OWNER OF LIFT ForYes elevators

(Marketing Executive)

(Authorized Signatory) (Marketing Manager)

Date: 03/04 /2025

\* **This offer is valid only for 30 days**.

INSTALLATION PERIOD AFTER COMPLETION OF CIVIL

& ELECTRICAL WORK. {{ip}} Weeks

FREE MAINTENANCE & WARRANTY 12 Months

WORK TO BE DONE BY THE CLIENT-

1. Store to be provided for material on site by you. If Store Room is Not Provided client is fully responsible for any theft or misplace of material.

2. Civil Work like Door frame fixing, Pocket Holes, Buffer column & Miscellaneous work by client

3. Electrical Cabling & provision of Light points in lift shaft & machine room is in Clients scope

NOTE:

WE HEREWITH REQUEST YOU, NOT TO GIVE BEARER CHEQUES, CASH PAYMENTS TO ANY PERSON FROM OUR ORGANISATION (EXCEPT Rs. 2,000.00 (INSPECTION FEES) PER LIFT.

All cheques / drafts must be drawn in favor of“YES ELEVATORS.”

This Offer from pages 1 to 4 accepted by you, shall constitute the contract between us to make this offer a legal and valid contract binding to both the parties. Break up for price and proof for tax payment cannot be provided.

1. If the 3- Phase power supply is not available within 10 days from date of delivery of material at your Site, the Payment of the contract amount should not be withheld, as it is not our responsibility.
2. For lift license customer need to provide all the document such as Owner applications, RCC & Architect certificate ,Approved plan.(these doc. are necessary for the license process)

**Accepted by**

**Proposed by**

OWNER OF LIFT

ForYes elevators

(Authorized Signatory)

(MarketingExecutive)

(Marketing Manager)